ЧехО.В.\_ІСЗП-93

14 июня 2020 г.

11:48

Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab2_print2.pcapng 196 всего пакетов, 4 показано
No.     Time           Source                Destination           Protocol Length Info
    109 40.160931      192.168.1.219         194.44.29.242         HTTP     542    GET /index.html HTTP/1.1 
Frame 109: 542 bytes on wire (4336 bits), 542 bytes captured (4336 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 194.44.29.242
    0100 .... = Version: 4
    .... 0101 = Header Length: 20 bytes (5)
    Differentiated Services Field: 0x00 (DSCP: CS0, ECN: Not-ECT)
    Total Length: 528
    Identification: 0x025b (603)
    Flags: 0x4000, Don't fragment
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (6)
    Header checksum: 0x0000 [validation disabled]
    [Header checksum status: Unverified]
    Source: 192.168.1.219
    Destination: 194.44.29.242
Transmission Control Protocol, Src Port: 51238, Dst Port: 80, Seq: 1, Ack: 1, Len: 476
    Source Port: 51238
    Destination Port: 80
    [Stream index: 7]
    [TCP Segment Len: 476]
    Sequence number: 1    (relative sequence number)
    Sequence number (raw): 2642532404
    [Next sequence number: 477    (relative sequence number)]
    Acknowledgment number: 1    (relative ack number)
    Acknowledgment number (raw): 1006725764
    1000 .... = Header Length: 32 bytes (8)
    Flags: 0x018 (PSH, ACK)
    Window size value: 16652
    [Calculated window size: 66608]
    [Window size scaling factor: 4]
    Checksum: 0xa4a4 [unverified]
    [Checksum Status: Unverified]
    Urgent pointer: 0
    Options: (12 bytes), No-Operation (NOP), No-Operation (NOP), Timestamps
    [SEQ/ACK analysis]
    [Timestamps]
    TCP payload (476 bytes)
Hypertext Transfer Protocol
    GET /index.html HTTP/1.1\r\n
    Host: 194.44.29.242\r\n
    Connection: keep-alive\r\n
    Cache-Control: max-age=0\r\n
    Upgrade-Insecure-Requests: 1\r\n
    User-Agent: Mozilla/5.0 (Windows NT 6.1; Win64; x64) AppleWebKit/537.36 (KHTML, like Gecko) Chrome/83.0.4103.97 Safari/537.36\r\n
    Accept: text/html,application/xhtml+xml,application/xml;q=0.9,image/webp,image/apng,*/*;q=0.8,application/signed-
exchange;v=b3;q=0.9\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: ru-RU,ru;q=0.9,en-US;q=0.8,en;q=0.7\r\n
    \r\n
    [Full request URI: http://194.44.29.242/index.html]
    [HTTP request 1/2]
    [Response in frame: 111]
    [Next request in frame: 113]
No.     Time           Source                Destination           Protocol Length Info
    111 40.165297      194.44.29.242         192.168.1.219         HTTP     476    HTTP/1.1 404 Not Found  (text/html)
Frame 111: 476 bytes on wire (3808 bits), 476 bytes captured (3808 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10), Dst: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d)
Internet Protocol Version 4, Src: 194.44.29.242, Dst: 192.168.1.219
    0100 .... = Version: 4
    .... 0101 = Header Length: 20 bytes (5)
    Differentiated Services Field: 0x00 (DSCP: CS0, ECN: Not-ECT)
    Total Length: 462
    Identification: 0x76e5 (30437)
    Flags: 0x4000, Don't fragment
    Fragment offset: 0
    Time to live: 59
    Protocol: TCP (6)
    Header checksum: 0x24a3 [validation disabled]
    [Header checksum status: Unverified]
    Source: 194.44.29.242
    Destination: 192.168.1.219
Transmission Control Protocol, Src Port: 80, Dst Port: 51238, Seq: 1, Ack: 477, Len: 410
    Source Port: 80
    Destination Port: 51238
    [Stream index: 7]
    [TCP Segment Len: 410]
    Sequence number: 1    (relative sequence number)
    Sequence number (raw): 1006725764
    [Next sequence number: 411    (relative sequence number)]
    Acknowledgment number: 477    (relative ack number)
    Acknowledgment number (raw): 2642532880
    1000 .... = Header Length: 32 bytes (8)
    Flags: 0x018 (PSH, ACK)
Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab2_print2.pcapng 196 всего пакетов, 4 показано
    Window size value: 243
    [Calculated window size: 15552]
    [Window size scaling factor: 64]
    Checksum: 0x3b1f [unverified]
    [Checksum Status: Unverified]
    Urgent pointer: 0
    Options: (12 bytes), No-Operation (NOP), No-Operation (NOP), Timestamps
    [SEQ/ACK analysis]
    [Timestamps]
    TCP payload (410 bytes)
Hypertext Transfer Protocol
    HTTP/1.1 404 Not Found\r\n
    Date: Fri, 12 Jun 2020 18:07:12 GMT\r\n
    Server: Apache\r\n
    Content-Length: 208\r\n
    Keep-Alive: timeout=15, max=100\r\n
    Connection: Keep-Alive\r\n
    Content-Type: text/html; charset=iso-8859-1\r\n
    \r\n
    [HTTP response 1/2]
    [Time since request: 0.004366000 seconds]
    [Request in frame: 109]
    [Next request in frame: 113]
    [Next response in frame: 114]
    [Request URI: http://194.44.29.242/index.html]
    File Data: 208 bytes
Line-based text data: text/html (7 lines)
No.     Time           Source                Destination           Protocol Length Info
    113 40.186592      192.168.1.219         194.44.29.242         HTTP     487    GET /favicon.ico HTTP/1.1 
Frame 113: 487 bytes on wire (3896 bits), 487 bytes captured (3896 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 194.44.29.242
    0100 .... = Version: 4
    .... 0101 = Header Length: 20 bytes (5)
    Differentiated Services Field: 0x00 (DSCP: CS0, ECN: Not-ECT)
    Total Length: 473
    Identification: 0x025d (605)
    Flags: 0x4000, Don't fragment
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (6)
    Header checksum: 0x0000 [validation disabled]
    [Header checksum status: Unverified]
    Source: 192.168.1.219
    Destination: 194.44.29.242
Transmission Control Protocol, Src Port: 51238, Dst Port: 80, Seq: 477, Ack: 411, Len: 421
    Source Port: 51238
    Destination Port: 80
    [Stream index: 7]
    [TCP Segment Len: 421]
    Sequence number: 477    (relative sequence number)
    Sequence number (raw): 2642532880
    [Next sequence number: 898    (relative sequence number)]
    Acknowledgment number: 411    (relative ack number)
    Acknowledgment number (raw): 1006726174
    1000 .... = Header Length: 32 bytes (8)
    Flags: 0x018 (PSH, ACK)
    Window size value: 16549
    [Calculated window size: 66196]
    [Window size scaling factor: 4]
    Checksum: 0xa46d [unverified]
    [Checksum Status: Unverified]
    Urgent pointer: 0
    Options: (12 bytes), No-Operation (NOP), No-Operation (NOP), Timestamps
    [SEQ/ACK analysis]
    [Timestamps]
    TCP payload (421 bytes)
Hypertext Transfer Protocol
    GET /favicon.ico HTTP/1.1\r\n
    Host: 194.44.29.242\r\n
    Connection: keep-alive\r\n
    Pragma: no-cache\r\n
    Cache-Control: no-cache\r\n
    User-Agent: Mozilla/5.0 (Windows NT 6.1; Win64; x64) AppleWebKit/537.36 (KHTML, like Gecko) Chrome/83.0.4103.97 Safari/537.36\r\n
    Accept: image/webp,image/apng,image/*,*/*;q=0.8\r\n
    Referer: http://194.44.29.242/index.html\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: ru-RU,ru;q=0.9,en-US;q=0.8,en;q=0.7\r\n
    \r\n
    [Full request URI: http://194.44.29.242/favicon.ico]
    [HTTP request 2/2]
    [Prev request in frame: 109]
    [Response in frame: 114]
No.     Time           Source                Destination           Protocol Length Info
    114 40.190855      194.44.29.242         192.168.1.219         HTTP     1506   HTTP/1.1 200 OK  (image/vnd.microsoft.icon)
Frame 114: 1506 bytes on wire (12048 bits), 1506 bytes captured (12048 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab2_print2.pcapng 196 всего пакетов, 4 показано
Ethernet II, Src: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10), Dst: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d)
Internet Protocol Version 4, Src: 194.44.29.242, Dst: 192.168.1.219
    0100 .... = Version: 4
    .... 0101 = Header Length: 20 bytes (5)
    Differentiated Services Field: 0x00 (DSCP: CS0, ECN: Not-ECT)
    Total Length: 1492
    Identification: 0x76e6 (30438)
    Flags: 0x4000, Don't fragment
    Fragment offset: 0
    Time to live: 59
    Protocol: TCP (6)
    Header checksum: 0x209c [validation disabled]
    [Header checksum status: Unverified]
    Source: 194.44.29.242
    Destination: 192.168.1.219
Transmission Control Protocol, Src Port: 80, Dst Port: 51238, Seq: 411, Ack: 898, Len: 1440
    Source Port: 80
    Destination Port: 51238
    [Stream index: 7]
    [TCP Segment Len: 1440]
    Sequence number: 411    (relative sequence number)
    Sequence number (raw): 1006726174
    [Next sequence number: 1851    (relative sequence number)]
    Acknowledgment number: 898    (relative ack number)
    Acknowledgment number (raw): 2642533301
    1000 .... = Header Length: 32 bytes (8)
    Flags: 0x018 (PSH, ACK)
    Window size value: 260
    [Calculated window size: 16640]
    [Window size scaling factor: 64]
    Checksum: 0x690a [unverified]
    [Checksum Status: Unverified]
    Urgent pointer: 0
    Options: (12 bytes), No-Operation (NOP), No-Operation (NOP), Timestamps
    [SEQ/ACK analysis]
    [Timestamps]
    TCP payload (1440 bytes)
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
    Date: Fri, 12 Jun 2020 18:07:12 GMT\r\n
    Server: Apache\r\n
    Last-Modified: Wed, 26 Dec 2018 13:49:37 GMT\r\n
    ETag: "131d-47e-57ded19cade40"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 1150\r\n
    Keep-Alive: timeout=15, max=99\r\n
    Connection: Keep-Alive\r\n
    Content-Type: image/vnd.microsoft.icon\r\n
    \r\n
    [HTTP response 2/2]
    [Time since request: 0.004263000 seconds]
    [Prev request in frame: 109]
    [Prev response in frame: 111]
    [Request in frame: 113]
    [Request URI: http://194.44.29.242/favicon.ico]
    File Data: 1150 bytes
Media Type
