ЧехО.В. ІСЗП-93

14 июня 2020 г.

11:43

Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab1_print3.pcapng 307 всего пакетов, 4 показано
No.     Time           Source                Destination           Protocol Length Info
    225 85.209558      192.168.1.219         128.119.245.12        HTTP     551    GET /wireshark-labs/INTRO-wireshark-file1.html
HTTP/1.1 
Packet comments
Frame 225: 551 bytes on wire (4408 bits), 551 bytes captured (4408 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 128.119.245.12
Transmission Control Protocol, Src Port: 50692, Dst Port: 80, Seq: 1, Ack: 1, Len: 485
Hypertext Transfer Protocol
    GET /wireshark-labs/INTRO-wireshark-file1.html HTTP/1.1\r\n
    Host: gaia.cs.umass.edu\r\n
    Connection: keep-alive\r\n
    Upgrade-Insecure-Requests: 1\r\n
    User-Agent: Mozilla/5.0 (Windows NT 6.1; Win64; x64) AppleWebKit/537.36 (KHTML, like Gecko) Chrome/83.0.4103.97 Safari/537.36\r\n
    Accept: text/html,application/xhtml+xml,application/xml;q=0.9,image/webp,image/apng,*/*;q=0.8,application/signed-
exchange;v=b3;q=0.9\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: ru-RU,ru;q=0.9,en-US;q=0.8,en;q=0.7\r\n
    \r\n
    [Full request URI: http://gaia.cs.umass.edu/wireshark-labs/INTRO-wireshark-file1.html]
    [HTTP request 1/2]
    [Response in frame: 229]
    [Next request in frame: 230]
No.     Time           Source                Destination           Protocol Length Info
    229 85.348009      128.119.245.12        192.168.1.219         HTTP     503    HTTP/1.1 200 OK  (text/html)
Frame 229: 503 bytes on wire (4024 bits), 503 bytes captured (4024 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10), Dst: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d)
Internet Protocol Version 4, Src: 128.119.245.12, Dst: 192.168.1.219
Transmission Control Protocol, Src Port: 80, Dst Port: 50692, Seq: 1, Ack: 486, Len: 437
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
    Date: Fri, 12 Jun 2020 15:46:20 GMT\r\n
    Server: Apache/2.4.6 (CentOS) OpenSSL/1.0.2k-fips PHP/7.4.6 mod_perl/2.0.11 Perl/v5.16.3\r\n
    Last-Modified: Fri, 12 Jun 2020 05:59:02 GMT\r\n
    ETag: "51-5a7dcc6240bea"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 81\r\n
    Keep-Alive: timeout=5, max=100\r\n
    Connection: Keep-Alive\r\n
    Content-Type: text/html; charset=UTF-8\r\n
    \r\n
    [HTTP response 1/2]
    [Time since request: 0.138451000 seconds]
    [Request in frame: 225]
    [Next request in frame: 230]
    [Next response in frame: 231]
    [Request URI: http://gaia.cs.umass.edu/wireshark-labs/INTRO-wireshark-file1.html]
    File Data: 81 bytes
Line-based text data: text/html (3 lines)
No.     Time           Source                Destination           Protocol Length Info
    230 85.393369      192.168.1.219         128.119.245.12        HTTP     483    GET /favicon.ico HTTP/1.1 
Frame 230: 483 bytes on wire (3864 bits), 483 bytes captured (3864 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 128.119.245.12
Transmission Control Protocol, Src Port: 50692, Dst Port: 80, Seq: 486, Ack: 438, Len: 417
Hypertext Transfer Protocol
    GET /favicon.ico HTTP/1.1\r\n
    Host: gaia.cs.umass.edu\r\n
    Connection: keep-alive\r\n
    User-Agent: Mozilla/5.0 (Windows NT 6.1; Win64; x64) AppleWebKit/537.36 (KHTML, like Gecko) Chrome/83.0.4103.97 Safari/537.36\r\n
    Accept: image/webp,image/apng,image/*,*/*;q=0.8\r\n
    Referer: http://gaia.cs.umass.edu/wireshark-labs/INTRO-wireshark-file1.html\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: ru-RU,ru;q=0.9,en-US;q=0.8,en;q=0.7\r\n
    \r\n
    [Full request URI: http://gaia.cs.umass.edu/favicon.ico]
    [HTTP request 2/2]
    [Prev request in frame: 225]
    [Response in frame: 231]
No.     Time           Source                Destination           Protocol Length Info
    231 85.517989      128.119.245.12        192.168.1.219         HTTP     549    HTTP/1.1 404 Not Found  (text/html)
Frame 231: 549 bytes on wire (4392 bits), 549 bytes captured (4392 bits) on interface \Device\NPF_{96132E11-79E5-48F2-
B0D9-1868991FA87E}, id 0
Ethernet II, Src: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10), Dst: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d)
Internet Protocol Version 4, Src: 128.119.245.12, Dst: 192.168.1.219
Transmission Control Protocol, Src Port: 80, Dst Port: 50692, Seq: 438, Ack: 903, Len: 483
Hypertext Transfer Protocol
    HTTP/1.1 404 Not Found\r\n
    Date: Fri, 12 Jun 2020 15:46:21 GMT\r\n
    Server: Apache/2.4.6 (CentOS) OpenSSL/1.0.2k-fips PHP/7.4.6 mod_perl/2.0.11 Perl/v5.16.3\r\n
    Content-Length: 209\r\n
    Keep-Alive: timeout=5, max=99\r\n
    Connection: Keep-Alive\r\n
    Content-Type: text/html; charset=iso-8859-1\r\n
    \r\n
Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab1_print3.pcapng 307 всего пакетов, 4 показано
    [HTTP response 2/2]
    [Time since request: 0.124620000 seconds]
    [Prev request in frame: 225]
    [Prev response in frame: 229]
    [Request in frame: 230]
    [Request URI: http://gaia.cs.umass.edu/favicon.ico]
    File Data: 209 bytes
Line-based text data: text/html (7 lines)
