ЧехО.В.\_ІСЗП-93

14 июня 2020 г.

11:58

Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab3_print4.pcapng 116 всего пакетов, 7 показано
No.     Time           Source                Destination           Protocol Length Info
     81 29.538444      192.168.1.219         192.168.1.1           DNS      73     Standard query 0xa38b A bitsy.mit.edu
Frame 81: 73 bytes on wire (584 bits), 73 bytes captured (584 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 192.168.1.1
User Datagram Protocol, Src Port: 52931, Dst Port: 53
    Source Port: 52931
    Destination Port: 53
    Length: 39
    Checksum: 0x8465 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 17]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0xa38b
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        bitsy.mit.edu: type A, class IN
            Name: bitsy.mit.edu
            [Name Length: 13]
            [Label Count: 3]
            Type: A (Host Address) (1)
            Class: IN (0x0001)
    [Response In: 82]
No.     Time           Source                Destination           Protocol Length Info
     82 29.539494      192.168.1.1           192.168.1.219         DNS      89     Standard query response 0xa38b A bitsy.mit.edu
A 18.0.72.3
Frame 82: 89 bytes on wire (712 bits), 89 bytes captured (712 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10), Dst: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d)
Internet Protocol Version 4, Src: 192.168.1.1, Dst: 192.168.1.219
User Datagram Protocol, Src Port: 53, Dst Port: 52931
    Source Port: 53
    Destination Port: 52931
    Length: 55
    Checksum: 0xd124 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 17]
    [Timestamps]
Domain Name System (response)
    Transaction ID: 0xa38b
    Flags: 0x8180 Standard query response, No error
    Questions: 1
    Answer RRs: 1
    Authority RRs: 0
    Additional RRs: 0
    Queries
        bitsy.mit.edu: type A, class IN
            Name: bitsy.mit.edu
            [Name Length: 13]
            [Label Count: 3]
            Type: A (Host Address) (1)
            Class: IN (0x0001)
    Answers
        bitsy.mit.edu: type A, class IN, addr 18.0.72.3
    [Request In: 81]
    [Time: 0.001050000 seconds]
No.     Time           Source                Destination           Protocol Length Info
     83 29.541053      192.168.1.219         18.0.72.3             DNS      82     Standard query 0x0001 PTR 3.72.0.18.in-addr.arpa
Frame 83: 82 bytes on wire (656 bits), 82 bytes captured (656 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 18.0.72.3
User Datagram Protocol, Src Port: 52932, Dst Port: 53
    Source Port: 52932
    Destination Port: 53
    Length: 48
    Checksum: 0x1cc8 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 18]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0x0001
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        3.72.0.18.in-addr.arpa: type PTR, class IN
            Name: 3.72.0.18.in-addr.arpa
            [Name Length: 22]
            [Label Count: 6]
Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab3_print4.pcapng 116 всего пакетов, 7 показано
            Type: PTR (domain name PoinTeR) (12)
            Class: IN (0x0001)
No.     Time           Source                Destination           Protocol Length Info
     86 31.547894      192.168.1.219         18.0.72.3             DNS      74     Standard query 0x0002 A www.aiit.or.kr
Frame 86: 74 bytes on wire (592 bits), 74 bytes captured (592 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 18.0.72.3
User Datagram Protocol, Src Port: 52933, Dst Port: 53
    Source Port: 52933
    Destination Port: 53
    Length: 40
    Checksum: 0x1cc0 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 19]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0x0002
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        www.aiit.or.kr: type A, class IN
            Name: www.aiit.or.kr
            [Name Length: 14]
            [Label Count: 4]
            Type: A (Host Address) (1)
            Class: IN (0x0001)
No.     Time           Source                Destination           Protocol Length Info
     90 33.549872      192.168.1.219         18.0.72.3             DNS      74     Standard query 0x0003 AAAA www.aiit.or.kr
Frame 90: 74 bytes on wire (592 bits), 74 bytes captured (592 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 18.0.72.3
User Datagram Protocol, Src Port: 52934, Dst Port: 53
    Source Port: 52934
    Destination Port: 53
    Length: 40
    Checksum: 0x1cc0 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 21]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0x0003
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        www.aiit.or.kr: type AAAA, class IN
            Name: www.aiit.or.kr
            [Name Length: 14]
            [Label Count: 4]
            Type: AAAA (IPv6 Address) (28)
            Class: IN (0x0001)
No.     Time           Source                Destination           Protocol Length Info
     94 35.553125      192.168.1.219         18.0.72.3             DNS      74     Standard query 0x0004 A www.aiit.or.kr
Frame 94: 74 bytes on wire (592 bits), 74 bytes captured (592 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 18.0.72.3
User Datagram Protocol, Src Port: 52935, Dst Port: 53
    Source Port: 52935
    Destination Port: 53
    Length: 40
    Checksum: 0x1cc0 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 23]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0x0004
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        www.aiit.or.kr: type A, class IN
            Name: www.aiit.or.kr
            [Name Length: 14]
            [Label Count: 4]
            Type: A (Host Address) (1)
            Class: IN (0x0001)
No.     Time           Source                Destination           Protocol Length Info
     99 37.554129      192.168.1.219         18.0.72.3             DNS      74     Standard query 0x0005 AAAA www.aiit.or.kr
Автоматически созданный замещающий текст: F:\КПІ\Семестр2\206 Комп'ютерні мережі\сети\лабораторн\dumps\lab3_print4.pcapng 116 всего пакетов, 7 показано
Frame 99: 74 bytes on wire (592 bits), 74 bytes captured (592 bits) on interface \Device\NPF_{96132E11-79E5-48F2-B0D9-1868991FA87E},
id 0
Ethernet II, Src: Micro-St_59:d7:7d (d4:3d:7e:59:d7:7d), Dst: ASUSTekC_db:a3:10 (54:a0:50:db:a3:10)
Internet Protocol Version 4, Src: 192.168.1.219, Dst: 18.0.72.3
User Datagram Protocol, Src Port: 52936, Dst Port: 53
    Source Port: 52936
    Destination Port: 53
    Length: 40
    Checksum: 0x1cc0 [unverified]
    [Checksum Status: Unverified]
    [Stream index: 24]
    [Timestamps]
Domain Name System (query)
    Transaction ID: 0x0005
    Flags: 0x0100 Standard query
    Questions: 1
    Answer RRs: 0
    Authority RRs: 0
    Additional RRs: 0
    Queries
        www.aiit.or.kr: type AAAA, class IN
            Name: www.aiit.or.kr
            [Name Length: 14]
            [Label Count: 4]
            Type: AAAA (IPv6 Address) (28)
            Class: IN (0x0001)
